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[bookmark: _GoBack]Preliminary procedure for the installation of a 4K7 sensor on a CX 2020 coaches.
· This is a mandatory modification for all the CX 2020 coaches.
· The defroster is equipped with a wrong 10K NTC sensor, which is incompatible with the control pot to regulate the defroster outlet temperature properly. A modification to a 4K7 NTC sensor is needed in order for the control pot to work properly. 
· VH ref sensor: 11259251
· An 8mm drill, hex key 2.5mm, a small screwdriver and some heat shrink tubing is needed for this procedure
· The procedure has been done on CX45 2020 #81513 and took approximately 15mins to complete.

Procedure
1) Remove the panel
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2) Drill a hole under the relay in the air duct
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3) Install the sensor
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4) Unscrew the panel with the 2.5mm hex key
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5) Remove the connector of the control pot
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6) Remove the wiring of the 10K sensor (white and brown, pin 5 and 6)
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7) Install wiring of new sensor
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8) Cut and protect the wiring ends of the 10K sensor
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9) Use tie wraps to fix the wiring of the sensor
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10) Remount the panels
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11) done
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